ESP Smart Planter – Documentation

Below are pictures of the custom PCB

A purple circuit board with yellow dots

Description automatically generatedA purple circuit board with yellow dots

Description automatically generated

# Hardware:

* ESP32 Devkit v1 (30 pins)
* PN532 RFID reader
* LDR
* (Capacitive) soil moisture sensor
* I2C 20x4 LCD
* Passive buzzer (or speaker)
* Ds18b20 soil temperature sensor
* BME280
* WS2812B LED (COB) strip
* 4-channel (5v) relay module
* Water pump (12v)
* Fan (12v)
* Power supply (12v)
* Step-down buck converter (12 -> 5v or a variable variant if it can output 5v)
* Wires

# The software:

* Grafana
* InfluxDB
* Python (MQTT -> InfluxDB)
* C++ firmware (for ESP32)

# The Grafana setup

In Grafana we add the data source ‘InfluxDB’ using the created credentials and localhost because the database is running on the same device as the Grafana server.

We can then use graphs to display the temperatures and light values as well as use labels to display statuses of, for example, the fan or lights.

The ESP32 sends the following data:

* Air temperature
* Soil temperature
* Soil moisture
* Light level
* Water level
* Fan status
* Lights status
* Pump Status
* Current target (which plant)

All of these datapoints are named appropriately in the influxdb.

# Installing the software and hardware

You can flash the ESP32 using PlatformIO or the Arduino IDE.  
Make sure to have all the required libraries installed!

All the required libraries are listed at the top of the C++ code.

If you are unsure of what pins to connect the sensors to, refer to the code or the provided schematic to see what sensors connect to which pins.

**Please make sure to change the WiFi SSID and Password BEFORE flashing the firmware to the board!**These can be found near the top of the code with the appropriately defined variables “WIFI\_SSID” and “WIFI\_PASSWORD”.